# How to display temperature measurement value and rules

## RTSP preview stream


RTSP url format：

rtsp://admin:abcd1234@10.14.136.101/Streaming/Channels/201/

admin:abcd1234 is the camera’s user name and password; 10.26.162.198 is the camera’s IP address;

201: The first number represents the thermal/visible channel, the second and third number represent the code stream.

2 is thermal channel, 01 is code stream. (so 101 is visible channel).



## Capture

Device protocol capture isapi url：

GET /ISAPI/Thermal/channels/<channelID>/thermometry/jpegPicWithAppendData?format=json

<channelID>：channel number，when <channelID> is 2 is as follows



Some operations that need to be done on the device side：

